Annex B
Technical Evaluation Methodology
Stage 1: Mandatory Requirements (Pass/Fail Basis):
All bids will first be evaluated against the Mandatory Requirements listed in Section 1.
Bidders who fail to meet any of the mandatory requirements will be disqualified and will not be considered for further evaluation.
Stage 2: Technical Evaluation (Pass/Fail Basis):
Only bidders who successfully meet all Mandatory Requirements will proceed to the Technical Evaluation stage. The Technical Evaluation will assess compliance with the requirements outlined in Annex A (Technical Specifications). Financial evaluation will be conducted separately. Bidders must achieve a “Pass” rating in the Technical Evaluation to be considered technically compliant.
Stage 3: Financial Evaluation:
Only bids determined to be technically compliant will proceed to the Financial Evaluation stage. The contract shall be awarded to the lowest priced technically compliant bidder, in accordance with the evaluation methodology specified in the RFQ. Failure to comply with any mandatory requirement shall render the bid non-responsive.
1. Mandatory Requirements
	S.Nu
	Requirement
	PASS/FAIL

	1
	Acceptance of UNHCR General Conditions of Contracts
	

	2
	Acceptance of UN Supplier Code of Conduct
	

	3
	Manufacturer Authorization (if bidder is not manufacturer)
	

	4
	Vendor Sanctions Screening Self-Declaration - Confirmation of Non-Inclusion on Vendor Sanctions Lists
	

	5
	Valid business license, Valid Tin Number and VAT Registration (if applicable)
	

	6
	Product brochure/catalogue
	

	7
	Warranty confirmation

	

	
	
	


2. Technical Offer (Pass/Fail)

	S. Nu 
	Requirement: Provision of the following Brands is a must deliver.
	PASS/FAIL

	1
	Model: PAA-36XiW-CTD, 200 m cable length.

Pass: If right model type quoted.
Fail: If others model types are quoted.
	

	2
	Model Type: 6466-M (NEW) AeroCone Rain Collector (VantagePro2) Base for Pole or Post mount 

Pass: If right model type quoted.
Fail: If other model types quoted.
	

	3
	Data Logger with: YDOC ML417 version 

Pass: If YDOC model quoted.
Fail: If other models quoted.
	

	4
	High Precision Digital Barometer: Version: YDOC ML-OI-BARO

Pass: If YDOC model quoted.
Fail: If other models quoted
	

	5
	VWR conduct port set phenome co 3100 H: 
Handheld device for measuring the conductivity (EC)

Pass: If portable and hand-carried devise is depicted
Fail: If not provided.
	

	6
	Eijkelkamp, level measuring device with frame 200m: Deep Water Meter 

Pass: If 200-meter measuring device is shown.
Fail: if not shown.
	

	7
	Bidders` supporting documents: Evidence submitted: Indicates whether catalogues, technical data sheets, certificates, test reports, have been fully provided or not. 

Pass: If all required supporting technical documents are provided.
Fail: If any required supporting documentation is missing or incomplete.
	

	8
	Compliance with Annex A: Fully Compliant / Partially Compliant / Non-Compliant

Pass: If fully compliant with all applicable technical requirements of Annex A.
Fail: If partially compliant or non-compliant.

	

	9
	Manufacturer’s Manual, showing the installation procedure for all appurtenances. 

Pass: If the manufacturer's manual(s) showing the installation procedures for all applicable equipment/appurtenances are submitted with the technical offer.
Fail: If not submitted or incomplete.
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