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Section III: Returnable Bidding Forms
eSourcing reference: ITB/2026/64017

Note to Bidders: The following returnable forms are part of this ITB and must be completed and returned by bidders as part of their Bid. Instructions to complete each Form are highlighted in blue in each Form. Please complete the Returnable Bidding Forms as instructed and return them as part of your bid by uploading them against their specific Document Checklist in the UNOPS eSourcing system.

This Section comprises the following Returnable Bidding Forms:
· Form A: Joint Venture Partner Information Form (optional)
· Form B: Bid Submission Form
· Form C: Price Schedule Form
· Form D: Technical Bid Form
· Form E: Performance Statement Form 
· Form F: Dealer or Manufacturer's Authorization Form 
In addition, bidders should submit the following additional documents.
· DRIVE Supplier Sustainability Questionnaire. (Should be completed online and is available under Forms section of the e-sourcing system) 
· National Business Registration Certificate or Valid Business Licences
· Copy of audited Financial statements (Balance sheets ) for the last two recent years
· [bookmark: _heading=h.gjdgxs]Manufacturer’s product data sheet /catalogue to support the bidder’s proposed product specification.
· [bookmark: _heading=h.30j0zll]Product Quality Certificate - ISO or  equivalent certification 

Form A: Joint Venture Partner Information Form / If Applicable/
The Bidder shall fill in this Form in accordance with the instructions indicated below.

ITB reference no: [insert ITB reference No.]
Name of Bidder: [insert name of bidder]
Date: [insert submission date]

To be completed and returned with your Bid if the Bid is submitted as a Joint Venture/Consortium/Association.

	JV / Consortium/ Association Information

	Name
	[complete]

	Names of each partner and contact information
(address, telephone numbers, fax numbers, e-mail address)  
	[complete]

	Name of leading partner (with authority to bind the JV, Consortium, Association during the Bidding process and, in the event a Contract is awarded, during contract execution)
	[complete]

	Proposed proportion of responsibilities between partners (in %) with indication of the type of the goods/services to be delivered by each
	[complete]



Signatures of all partners of the JV: 	 

We hereby confirm that if the contract is awarded, all parties of the Joint Venture/Consortium/Association shall be jointly and severally liable to UNOPS for the fulfilment of the provisions of the Contract.


Name of partner: ________________________		Name of partner: _________________________ 

Signature: ______________________________		Signature: _______________________________

Date: _______________________			Date:  ________________________



Name of partner: ________________________		Name of partner: _________________________ 

Signature: ______________________________		Signature: _______________________________

Date: _______________________			Date:  ________________________



Form B: Bid Submission Form

Bidders are requested to complete this form, sign it and return it as part of their bid submission. The bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted. 

Date: [Insert submission date]

Subject:  Re-Bid for the supply of [Insert a brief description of goods/services] in [Name of country/city], ITB Case No. [Insert ITB ref number], dated [insert date]

We, the undersigned, declare that: 

a. We have examined and have no reservations to the bidding documents, including amendments No.: [Insert the number and issuing date of each amendment]; 
b. We offer to supply in conformity with the bidding documents, including the UNOPS General Conditions of Contract, and in accordance with the delivery schedules specified in the Schedule of Requirements
c. The total price of our bid, excluding any discounts offered in item (d) below, is: [Insert the total bid price in words and figures, indicating the various amounts and the respective currencies];
d. The discounts offered and the methodology for their application are:
· Discounts: If our bid is accepted, the following discounts shall apply. [Specify in detail each discount offered and the specific item of the Schedule of Requirements to which it applies, including if applicable discounts for accelerated payment.]
· Methodology of application of the discounts: The discounts shall be applied using the following method: [Specify in detail the method that shall be used to apply the discounts];
e. Our bid shall be valid for the period of time of [insert number of days which shall not be less than the specified in the Tender Particulars section, Period of Validity of Bids] from the date fixed for the bid submission deadline as set out in the ITB, and it shall remain binding upon us and may be accepted at any time before the expiration of that period;
f. If our bid is accepted, and if so requested in the Tender Particulars section, we commit to obtain a performance security in accordance with Instructions to Bidders Article 34 and the General Conditions of Contract;
g. We have no conflict of interest in any activity that would put it, if selected for this assignment, in a conflict of interest with UNOPS;
h. We have not declared bankruptcy, are not involved in bankruptcy or receivership proceedings, and there is no judgement or pending legal action against them that could impair their operations in the foreseeable future;

i. Our firm confirms that the Bidder and sub-contractors have not been associated, or had been involved in any way, directly or indirectly, with the preparation of the design, terms of references and/or other documents used as a part of this solicitation;
j. We embrace the principles of the United Nations Supplier Code of Conduct and adhere to the principles of the United Nations Global Compact;
k. Our firm, its affiliates or subsidiaries – including any subcontractors or suppliers for any part of the contract – has not been declared ineligible by UNOPS, nor is included in the suspended/ineligibility list of the UN/PD, other UN Agencies, the UN Security Council, and the World Bank, in accordance with Instructions to Bidders Article 4, Eligibility;
l. We have not offered and will not offer fees, gifts and/or favours of kind in exchange for this ITB and will not engage in any such activity during the performance of any contract awarded; 
m. We understand that you are not bound to accept the lowest evaluated bid or any other bid that you may receive.
I, the undersigned, certify that I am duly authorised by [insert full name of bidder] to sign this bid and bind [insert full name of bidder] should UNOPS accept this bid: 


[Stamp form of bid with official stamp of the bidder]
Name	: _____________________________________________________________

Title	: _____________________________________________________________

Date	: _____________________________________________________________

Signature	: _____________________________________________________________



Form C: Price Schedule Form
Bidders must offer 100% of the items specified under each lot   and 100% of the quantities specified.  N.B UNOPS reserves the right to award the contract on either FCA or DAP INCOTERM basis at the time of award in the best interest of UNOPS. 

Lot 1-Drilling Rig 600mtr with Booster,compressor, tools ,accessories & spareparts-4 Units-with Full accessories
ITB reference no: [insert ITB reference No.]
Name of Bidder: [insert name of bidder]

Bidders shall fill in these Price Schedule Forms in accordance with the instructions indicated.  
Bid Summary

It. No.	Description	UoM	Qty (a)	Currency USD
				Unit price FCA (b)	Total price FCA (c)= (a)x(b)
1	Complete set of Drilling rig 600mtr with truck, Mast, Outrigger, welder- generator, deckengine and compressor, 	Set	4		
2	Booster machine with all its accessories and  spare parts	Set	4		
3	Mobile Compressor with all its accessories and spare parts 	Set	4		
Drilling Spareparts, Tools and Accessories for 600Mtr Drilling Rig
No.	Description	Unit	Qty		
1	DRILL PIPE 5", length 6 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	440		
2	DRILL PIPE 5", length 3 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	8		
3	DRILL COLLAR 6" (152,4 mm) Length 6 m, thread 4 1/2" API REG, internal diameter 50 mm, wrench on both ends and thread protection with non-return valve which are replaceable	PCS	8		
4	DRILL COLLAR 8" (203.2 mm) Length 6 m, thread 6 5/8" API REG, internal diameter 90 mm, wrench on both ends and thread protection with non-return valve which are replaceable	PCS	8		
5	Spiral stabilizers 12 1/4" - body 8"x2 m with 6 5/8"API REG (B))x(P), wrench recess on both ends and hard thread protection	PCS	4		
6	Spiral stabilizers 14" (350 mm) - body 8" (203 mm) x1,5 m with 6 5/8"API REG (B))x(P), internal hole diameter 80 mm	PCS	8		
7	Cross over sub 4 1/2" API IF box x 3 1/2" API IF pin, length 300 mm	PCS	8		
8	Cross over sub 4 1/2" API IF box x 6 5/8"	PCS	4		
9	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 3 1/2" API IF, load capacity 3200 Kg	PCS	8		
10	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 6 5/8" API IF, load capacity 4600 Kg	PCS	8		
11	HOISTING PLUG, BOX type for drill rods with threads 4 1/2" API REG, load capacity 2000 Kg	PCS	8		
12	HOISTING PLUG, BOX type for drill rods with threads 6 5/8" API REG, load capacity 2000 Kg	PCS	4		
13	HOISTING PLUG, Box type, for drilling bits with threads 7 5/8" API REG, load capacity 4600 Kg	PCS	4		
14	SUB, 3 1/2" API IF BOX , 4 1/2" API REG BOX	PCS	8		
15	SUB, 6 5/8" API REG PIN, 4 1/2" API REG BOX	PCS	8		
16	SUB, 6 5/8" API REG BOX, 4 1/2" API REG BOX	PCS	8		
17	SUB, 6 5/8" API REG BOX, 6 5/8" API REG BOX	PCS	16		
18	SUB, 6 5/8" API REG BOX, 7 5/8" API REG BOX	PCS	8		
19	SUB, 4 1/2" API REG BOX, 4 1/2" API REG BOX	PCS	4		
20	Tricone 12 1/4" (311.1 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "4", for medium-hard formation and 3 jet flushing	PCS	8		
21	Tricone 14 3/4" (374.6 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing	PCS	8		
22	TRICONE 17 1/2" (444.5 mm) IADC 535, TCI inserts, thread 7 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing	PCS	8		
23	TRICONE 9 7/8" (250,8 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for hard formation and central flushing	PCS	8		
24	TRICONE 9 7/8" (250,8 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	8		
25	TRICONE 12 1/4" (311,1 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	8		
26	TRICONE 14 3/4" (375 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	8		
27	TRICONE 17 1/2" (444,5 mm) IADC 211, tooth type, thread 7 5/8" API REG Pin, for soft formation and with central flushing	PCS	8		
28	Drag bit 10 5/8" (270 mm), thread 4 1/2" API REG Pin	PCS	8		
29	Drag bit 12 1/4" (311 mm), thread 3 1/2" API REG Pin	PCS	4		
30	Drag bit 14 3/4" (375 mm), thread 4 1/2" API REG Pin	PCS	4		
31	Drag bit 17 1/2" (444,5 mm), thread 6 5/8" API REG Pin	PCS	4		
32	DOWN THE HOLE HAMMER 8" with shank DHD 380 and thread 4 1/2" API REG Pin	PCS	4		
33	DOWN THE HOLE HAMMER 10" with shank SD 10 and thread 6 5/8" API REG Pin	PCS	8		
34	DOWN THE HOLE HAMMER 12" with shank SD 12 and thread 6 5/8" API REG Pin	PCS	8		
35	BIT 121/4" (311 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	8		
36	BIT 121/4" (311 mm) concave face for DTH Hammer 12" with shank SD 10	PCS	8		
37	BIT 15" (311 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	8		
38	BIT 15" (311 mm) concave face for DTH Hammer 12" with shank SD 10	PCS	8		
39	BIT 10" (254 mm) concave face for DTH Hammer 10" with shank DHD 380	PCS	4		
40	BIT 10" (254 mm) concave face for DTH Hammer 12" with shank DHD 380	PCS	8		
41	BIT 8 1/2" (216 mm) concave face for DTH Hammer 10" with shank DHD 380	PCS	8		
42	BIT 17 1/2" (445 mm) concave face for DTH Hammer with shank DHD 380 appropriate for the bit.	PCS	8		
43	BIT 201/2" (520.7 mm) concave face for DTH Hammer with shank DHD 380 appropriate for the bit.	PCS	8		
44	Grinding wheel (bit) for the above grinder( Row#32-40) to suit all the insert sizes	Set	4		
45	Bit Breaker for tricone diameter 20 1/2	Pcs	4		
46	Bit Breaker for tricone diameter 17 ½”	PCS	4		
47	Bit Breaker for tricone diameter 14 3/4"	PCS	4		
48	Bit Breaker for tricone diameter 12 1/4"	PCS	4		
49	Bit Breaker for tricone diameter 10 5/8"	PCS	4		
50	Bit Breaker for tricone diameter 9 7/8"	PCS	4		
51	Steel Casing elevators 6 5/8"	PCS	8		
52	Steel Casing elevators 8 5/8"	PCS	8		
53	Steel Casing elevators 10 3/4"	PCS	8		
54	Steel Casing elevators 17 1/2"	PCS	8		
55	Steel Casing elevators 201/2"	PCS	8		
56	Steel Casing elevators 121/2"	PCS	8		
57	Steel Casing elevators 141/2"	PCS	8		
58	Casing clamp and slips for steel casing 6 5/8", max capacity 55 tons	PCS	4		
59	Casing clamp and slips for steel casing 8 5/8", max capacity 20 tons	PCS	4		
60	Casing clamp and slips for steel casing 10 3/4", max capacity 55 tons	PCS	4		
61	Casing clamp and slips for steel casing 12 3/4", max capacity 55 tons	Pcs	4		
62	Casing clamp and slips for steel casing 14 3/4", max capacity 55 tons	Pcs	4		
63	Casing Elevators for 6 5/8" PVC Casing	PCS	4		
64	Casing Elevators for 8 5/8" PVC Casing	PCS	4		
65	Casing Elevators for 10 3/4" PVC Casing	PCS	4		
66	Kit of casing clamp for 6 5/8", " PVC casing flush joint type (n°1 each diameter)	PCS	4		
67	Kit of casing clamp for 8 5/8", PVC casing flush joint type (n°1 each diameter)	PCS	4		
68	Kit of casing clamp for 10 3/4" PVC casing flush joint type (n°1 each diameter)	PCS	4		
69	SHOCK ABSORBER for DTH HAMMER 8", thread 4 1/2" API Reg	PCS	8		
70	SHOCK ABSORBER for DTH HAMMER 10", thread 6 5/8" API Reg	PCS	8		
71	SHOCK ABSORBER for DTH HAMMER 12", thread 6 5/8" API Reg	PCS	8		
72	Loading kit (2 cable rings plus 2 shackles) for casing elevator, max capacity 30 tons	Set	4		
73	JET HOOPER MIXER: Jet hopper mixer 60 liters with accessories.	Pcs	4		
74	Foldable Water tight canvas TANK FOR FOAM and WATER: Minimum Capacity of 4000litrs,	with air agitation for polymer mixing.	Pcs	4		
75	HAND OPERATED manual OIL & FUEL pump	Filling pump with filter for oil & fuel, actioned manually.	Pcs	4		
76	Fishing tools with:	= taper tap for 3 1/2" API IF Box drill pipe, -1pcs each	= die collar for 3 1/2" API IF Box drill pipe, -1pcseach	= fishing magnet OD 6 1/2" with pulling capacity 400kg-1pcseach	Set	4		
77	Chain Tong for Casing 12" (Gr. 35) - 8" (Gr. 34) - 6" (Gr. 33 1/2")	Set	4		
78	Shackle AR Omega D+C 17 Tons	Pcs	8		
79	Shackle AR Omega D+C 25 Tons	Pcs	8		
80	Wire sling 12 mm , 6 m length - Sling Type Eye/Eye	Pcs	4		
81	Wire sling 10 mm , 3 m length - Sling Type Eye/Eye	Pcs	4		
82	Wire sling 10 mm 1.5 m length - Sling Type Eye/Eye	Pcs	4		
83	Sliding caliper 0-300 mm	Pcs	4		
84	Nipper 150 mm	Pcs	4		
85	Top adaptor spanner for DTH hammer cylinder 8"	Pcs	4		
86	TOP ADAPTOR SPANNER	Pcs	4		
87	14" BIT SPANNER	Pcs	4		
88	12" BIT SPANNER	Pcs	4		
89	10" BIT SPANNER	Pcs	4		
90	8" BIT SPANNER	Pcs	4		
91	17 1/2" Bit spanner	Pcs	4		
92	201/2" Bit spanner	Pcs	4		
93	Standard safety equipment for a crew of six members	Set	24		
	TOOL BOX & MAINTENANCE KIT for 600Mtr				
	Description	Unit	Qty		
1	Slogging Wrenches: Open-end and 12-point box ends (up to 3" or 75mm) for hammer-tightening structural bolts.	set	4		
2	Heavy-Duty Socket Set: 3/4" and 1" drive sets for high-torque applications.	set	4		
3	Torque Multipliers: Essential for reaching the high foot-pound requirements of flange bolts and mounting hardware.	set	4		
4	Large Pipe Wrenches: 18 ", 24", 36", and 48" (Rigid-style) for mud lines and drill floor piping.(each size 1 pcs)	set	4		
5	Impact Wrenches: Pneumatic 1" drive impact tools for fast removal of heavy covers and guards.	pcs	4		
6	Pressure Gauges: 0–5,000 psi (350 bar) digital or liquid-filled gauges with quick-connect fittings.	pcs	4		
7	Hydraulic Hose Crimper & Cutter: For on-site repairs of auxiliary lines.	set	4		
8	Hydraulic Jacks: 20-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	4		
9	Hydraulic Jacks: 50-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	4		
10	Fluid Sampling Kit: To monitor hydraulic oil cleanliness and prevent pump cavitation.-	set	4		
11	Digital Mustimeter: CAT IV rated (e.g., Fluke 87V or equivalent) for troubleshooting high-voltage power systems.	pcs	4		
12	Clamp Meter: To measure high amperage on mud pump motors and the drawworks.	pcs	4		
13	Insulation Tester (Megohmmeter): For testing motor windings and cable integrity against the rig ground.	pcs	4		
14	Precision Screwdriver Set: For PLC (Programmable Logic Controller) and control board wiring.	set	4		
15	Infrared (Thermal) Camera: To detect hot spots in electrical panels or overheating bearings before they fail.	set	4		
16	High-Pressure Grease Gun: Manual and battery-powered (18V) for the dozens of grease points on the mast and swivel.	pcs	4		
17	Lubrication Chart: Specific to your rig model, tracking hours vs. grease type (EP2, High-Temp, etc.).	pcs	4		
18	Oil Filter Wrenches: Large strap-style wrenches for engine and hydraulic return filters.	pcs	4		
19	Parts Washer/Solvent Kit: For cleaning shale shaker screens and fouled valves.	pcs	4		
Spare parts to be supplied for the 600m Drilling Rig
No.	Description	Unit	Qty		
1	Truck air filter set	pcs	20		
2	Truck oil filter set	pcs	40		
3	Truck fuel filter set	pcs	40		
4	Deck engine air filters	pcs	20		
5	Deck engine oil filters	pcs	40		
6	Deck engine fuel filters	pcs	40		
7	welder Generator air filters	pcs	20		
8	welder Generator oil filters	pcs	40		
9	welder Generator fuel filters	pcs	40		
10	Booster Engine air filters	pcs	20		
11	Booster Engine oil filters	pcs	40		
12	Booster Engine fuel filters	pcs	40		
13	V-Belts: A matched set for the cooling fans and auxiliary pumps for the primary power unit(Deck Engine, Carrier Truck Engine, welder Generator, booster Engine)- 2Pcs for Each	Set	4		
14	Hydraulic oil filter elements set- for the hydraulic system	set	8		
15	Wheel and master cylinder repair kit & brake lining	pcs	20		
16	All hydraulic lines and hoses fitting seals (Washers and seal kit)	kit	40		
17	Kit for air compressor	kit	40		
18	Flange and O-Ring Kit: A comprehensive set of Viton O-rings, SAE, and Metric seals.	set	16		
19	Mud seal "V"	pcs	8		
20	Pack of gasket for the Power units(Deck Engine, Carrier Truck Engine, welder Generator, booster Engine)- 1 set for each	Set	4		
21	Shear Pins & Fuses: For mechanical and electrical overload protection.	set	4		
22	BOP Seal Kit: Critical for maintaining the Blowout Preventer pressure integrity	set	4		
	Sub Total FCA 	
	Freight Cost ( For the Rigs + Spareparts+ Accessories +Tools)	
	Insurance cost	
	Customs clearance, and offloading cost  	
	PDI for the Truck  	
	Installation, and commissioning  of the Rig(The awarded bidder is required to commission the drilling Rig by drilling a 600mtr long drilling well) as per the required depth of max 600Mtr at final destination (Afar, Dire Dawa Administration ,Somali & Oromia) 	
	Training cost  at the Four Locations (Afar, Dire Dawa Administration Somali & Oromia) for 10 persons per / location for a duration of 20days-for each of the regions however the training is going to be made simultaneously. The Total Training Period for all the Regions should not exceed 30Days	
	Bidder’s Total prices DAP- MILS Warehouse (Total FCA+Freight Cost+ Insurance cost+ Customs clearance and offloading cost, PDI Cost , Installation , commissioning and Training Cost  at final destination)  	















Lot 2-Drilling Rig 600mtr with Booster,compressor, tools ,accessories & spareparts-4 Units-with limited accessories

Bid Summary

It. No.	Description	UoM	Qty (a)	Currency USD
				Unit price FCA (b)	Total price FCA (c)= (a)x(b)
1	Complete set of Drilling rig 600mtr with truck, Mast, Outrigger, welder- generator, deckengine and compressor, 	Set	4		
2	Booster machine with all its accessories and  spare parts	Set	4		
3	Mobile Compressor with all its accessories and spare parts 	Set	4		
Drilling Spareparts, Tools and Accessories for 600Mtr Drilling Rig
No.	Description	Unit	Qty		
1	DRILL PIPE 5", length 6 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	400		
2	DRILL PIPE 5", length 3 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	4		
3	DRILL COLLAR 6" (152,4 mm) Length 6 m, thread 4 1/2" API REG, internal diameter 50 mm, wrench on both ends and thread protection with non-return valve which are replaceable	PCS	4		
4	DRILL COLLAR 8" (203.2 mm) Length 6 m, thread 6 5/8" API REG, internal diameter 90 mm, wrench on both ends and thread protection with non-return valve which are replaceable	PCS	4		
5	Spiral stabilizers 12 1/4" - body 8"x2 m with 6 5/8"API REG (B))x(P), wrench recess on both ends and hard thread protection	PCS	4		
6	Spiral stabilizers 14" (350 mm) - body 8" (203 mm) x1,5 m with 6 5/8"API REG (B))x(P), internal hole diameter 80 mm	PCS	4		
7	Cross over sub 4 1/2" API IF box x 3 1/2" API IF pin, length 300 mm	PCS	4		
8	Cross over sub 4 1/2" API IF box x 6 5/8"	PCS	4		
9	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 3 1/2" API IF, load capacity 3200 Kg	PCS	4		
10	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 6 5/8" API IF, load capacity 4600 Kg	PCS	4		
11	HOISTING PLUG, BOX type for drill rods with threads 4 1/2" API REG, load capacity 2000 Kg	PCS	4		
12	HOISTING PLUG, BOX type for drill rods with threads 6 5/8" API REG, load capacity 2000 Kg	PCS	4		
13	HOISTING PLUG, Box type, for drilling bits with threads 7 5/8" API REG, load capacity 4600 Kg	PCS	4		
14	SUB, 3 1/2" API IF BOX , 4 1/2" API REG BOX	PCS	4		
15	SUB, 6 5/8" API REG PIN, 4 1/2" API REG BOX	PCS	4		
16	SUB, 6 5/8" API REG BOX, 4 1/2" API REG BOX	PCS	4		
17	SUB, 6 5/8" API REG BOX, 6 5/8" API REG BOX	PCS	8		
18	SUB, 6 5/8" API REG BOX, 7 5/8" API REG BOX	PCS	4		
19	SUB, 4 1/2" API REG BOX, 4 1/2" API REG BOX	PCS	4		
20	Tricone 12 1/4" (311.1 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "4", for medium-hard formation and 3 jet flushing	PCS	4		
21	Tricone 14 3/4" (374.6 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing	PCS	4		
22	TRICONE 17 1/2" (444.5 mm) IADC 535, TCI inserts, thread 7 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing	PCS	4		
23	TRICONE 9 7/8" (250,8 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for hard formation and central flushing	PCS	4		
24	TRICONE 9 7/8" (250,8 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	4		
25	TRICONE 12 1/4" (311,1 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	4		
26	TRICONE 14 3/4" (375 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	4		
27	TRICONE 17 1/2" (444,5 mm) IADC 211, tooth type, thread 7 5/8" API REG Pin, for soft formation and with central flushing	PCS	4		
28	Drag bit 10 5/8" (270 mm), thread 4 1/2" API REG Pin	PCS	4		
29	Drag bit 12 1/4" (311 mm), thread 3 1/2" API REG Pin	PCS	4		
30	Drag bit 14 3/4" (375 mm), thread 4 1/2" API REG Pin	PCS	4		
31	Drag bit 17 1/2" (444,5 mm), thread 6 5/8" API REG Pin	PCS	4		
32	DOWN THE HOLE HAMMER 8" with shank DHD 380 and thread 4 1/2" API REG Pin	PCS	4		
33	DOWN THE HOLE HAMMER 10" with shank SD 10 and thread 6 5/8" API REG Pin	PCS	4		
34	DOWN THE HOLE HAMMER 12" with shank SD 12 and thread 6 5/8" API REG Pin	PCS	4		
35	BIT 121/4" (311 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	4		
36	BIT 121/4" (311 mm) concave face for DTH Hammer 12" with shank SD 10	PCS	4		
37	BIT 15" (311 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	4		
38	BIT 15" (311 mm) concave face for DTH Hammer 12" with shank SD 10	PCS	4		
39	BIT 10" (254 mm) concave face for DTH Hammer 10" with shank DHD 380	PCS	4		
40	BIT 10" (254 mm) concave face for DTH Hammer 12" with shank DHD 380	PCS	4		
41	BIT 8 1/2" (216 mm) concave face for DTH Hammer 10" with shank DHD 380	PCS	4		
42	BIT 17 1/2" (445 mm) concave face for DTH Hammer with shank DHD 380 appropriate for the bit.	PCS	4		
43	BIT 201/2" (520.7 mm) concave face for DTH Hammer with shank DHD 380 appropriate for the bit.	PCS	4		
44	Grinding wheel (bit) for the above grinder( Row#32-40) to suit all the insert sizes	Set	4		
45	Bit Breaker for tricone diameter 20 1/2	Pcs	4		
46	Bit Breaker for tricone diameter 17 ½”	PCS	4		
47	Bit Breaker for tricone diameter 14 3/4"	PCS	4		
48	Bit Breaker for tricone diameter 12 1/4"	PCS	4		
49	Bit Breaker for tricone diameter 10 5/8"	PCS	4		
50	Bit Breaker for tricone diameter 9 7/8"	PCS	4		
51	Steel Casing elevators 6 5/8"	PCS	4		
52	Steel Casing elevators 8 5/8"	PCS	4		
53	Steel Casing elevators 10 3/4"	PCS	4		
54	Steel Casing elevators 17 1/2"	PCS	4		
55	Steel Casing elevators 201/2"	PCS	4		
56	Steel Casing elevators 121/2"	PCS	4		
57	Steel Casing elevators 141/2"	PCS	4		
58	Casing clamp and slips for steel casing 6 5/8", max capacity 55 tons	PCS	4		
59	Casing clamp and slips for steel casing 8 5/8", max capacity 20 tons	PCS	4		
60	Casing clamp and slips for steel casing 10 3/4", max capacity 55 tons	PCS	4		
61	Casing clamp and slips for steel casing 12 3/4", max capacity 55 tons	Pcs	4		
62	Casing clamp and slips for steel casing 14 3/4", max capacity 55 tons	Pcs	4		
63	Casing Elevators for 6 5/8" PVC Casing	PCS	4		
64	Casing Elevators for 8 5/8" PVC Casing	PCS	4		
65	Casing Elevators for 10 3/4" PVC Casing	PCS	4		
66	Kit of casing clamp for 6 5/8", " PVC casing flush joint type (n°1 each diameter)	PCS	4		
67	Kit of casing clamp for 8 5/8", PVC casing flush joint type (n°1 each diameter)	PCS	4		
68	Kit of casing clamp for 10 3/4" PVC casing flush joint type (n°1 each diameter)	PCS	4		
69	SHOCK ABSORBER for DTH HAMMER 8", thread 4 1/2" API Reg	PCS	4		
70	SHOCK ABSORBER for DTH HAMMER 10", thread 6 5/8" API Reg	PCS	4		
71	SHOCK ABSORBER for DTH HAMMER 12", thread 6 5/8" API Reg	PCS	4		
72	Loading kit (2 cable rings plus 2 shackles) for casing elevator, max capacity 30 tons	Set	4		
73	JET HOOPER MIXER: Jet hopper mixer 60 liters with accessories.	Pcs	4		
74	Foldable Water tight canvas TANK FOR FOAM and WATER: Minimum Capacity of 4000litrs,	with air agitation for polymer mixing.	Pcs	4		
75	HAND OPERATED manual OIL & FUEL pump	Filling pump with filter for oil & fuel, actioned manually.	Pcs	4		
76	Fishing tools with:	= taper tap for 3 1/2" API IF Box drill pipe, -1pcs each	= die collar for 3 1/2" API IF Box drill pipe, -1pcseach	= fishing magnet OD 6 1/2" with pulling capacity 400kg-1pcseach	Set	4		
77	Chain Tong for Casing 12" (Gr. 35) - 8" (Gr. 34) - 6" (Gr. 33 1/2")	Set	4		
78	Shackle AR Omega D+C 17 Tons	Pcs	4		
79	Shackle AR Omega D+C 25 Tons	Pcs	4		
80	Wire sling 12 mm , 6 m length - Sling Type Eye/Eye	Pcs	4		
81	Wire sling 10 mm , 3 m length - Sling Type Eye/Eye	Pcs	4		
82	Wire sling 10 mm 1.5 m length - Sling Type Eye/Eye	Pcs	4		
83	Sliding caliper 0-300 mm	Pcs	4		
84	Nipper 150 mm	Pcs	4		
85	Top adaptor spanner for DTH hammer cylinder 8"	Pcs	4		
86	TOP ADAPTOR SPANNER	Pcs	4		
87	14" BIT SPANNER	Pcs	4		
88	12" BIT SPANNER	Pcs	4		
89	10" BIT SPANNER	Pcs	4		
90	8" BIT SPANNER	Pcs	4		
91	17 1/2" Bit spanner	Pcs	4		
92	201/2" Bit spanner	Pcs	4		
93	Standard safety equipment for a crew of six members	Set	24		
	TOOL BOX & MAINTENANCE KIT for 600Mtr				
	Description	Unit	Qty		
1	Slogging Wrenches: Open-end and 12-point box ends (up to 3" or 75mm) for hammer-tightening structural bolts.	set	4		
2	Heavy-Duty Socket Set: 3/4" and 1" drive sets for high-torque applications.	set	4		
3	Torque Multipliers: Essential for reaching the high foot-pound requirements of flange bolts and mounting hardware.	set	4		
4	Large Pipe Wrenches: 18 ", 24", 36", and 48" (Rigid-style) for mud lines and drill floor piping.(each size 1 pcs)	set	4		
5	Impact Wrenches: Pneumatic 1" drive impact tools for fast removal of heavy covers and guards.	pcs	4		
6	Pressure Gauges: 0–5,000 psi (350 bar) digital or liquid-filled gauges with quick-connect fittings.	pcs	4		
7	Hydraulic Hose Crimper & Cutter: For on-site repairs of auxiliary lines.	set	4		
8	Hydraulic Jacks: 20-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	4		
9	Hydraulic Jacks: 50-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	4		
10	Fluid Sampling Kit: To monitor hydraulic oil cleanliness and prevent pump cavitation.-	set	4		
11	Digital Mustimeter: CAT IV rated (e.g., Fluke 87V or equivalent) for troubleshooting high-voltage power systems.	pcs	4		
12	Clamp Meter: To measure high amperage on mud pump motors and the drawworks.	pcs	4		
13	Insulation Tester (Megohmmeter): For testing motor windings and cable integrity against the rig ground.	pcs	4		
14	Precision Screwdriver Set: For PLC (Programmable Logic Controller) and control board wiring.	set	4		
15	Infrared (Thermal) Camera: To detect hot spots in electrical panels or overheating bearings before they fail.	set	4		
16	High-Pressure Grease Gun: Manual and battery-powered (18V) for the dozens of grease points on the mast and swivel.	pcs	4		
17	Lubrication Chart: Specific to your rig model, tracking hours vs. grease type (EP2, High-Temp, etc.).	pcs	4		
18	Oil Filter Wrenches: Large strap-style wrenches for engine and hydraulic return filters.	pcs	4		
19	Parts Washer/Solvent Kit: For cleaning shale shaker screens and fouled valves.	pcs	4		
Spare parts to be supplied for the 600m Drilling Rig
No.	Description	Unit	Qty		
1	Truck air filter set	pcs	8		
2	Truck oil filter set	pcs	20		
3	Truck fuel filter set	pcs	20		
4	Deck engine air filters	pcs	8		
5	Deck engine oil filters	pcs	20		
6	Deck engine fuel filters	pcs	20		
7	welder Generator air filters	pcs	8		
8	welder Generator oil filters	pcs	20		
9	welder Generator fuel filters	pcs	20		
10	Booster Engine air filters	pcs	8		
11	Booster Engine oil filters	pcs	20		
12	Booster Engine fuel filters	pcs	20		
13	V-Belts: A matched set for the cooling fans and auxiliary pumps for the primary power unit(Deck Engine, Carrier Truck Engine, welder Generator, booster Engine)- 2Pcs for Each	Set	4		
14	Hydraulic oil filter elements set- for the hydraulic system	set	4		
15	Wheel and master cylinder repair kit & brake lining	pcs	8		
16	All hydraulic lines and hoses fitting seals (Washers and seal kit)	kit	20		
17	Kit for air compressor	kit	20		
18	Flange and O-Ring Kit: A comprehensive set of Viton O-rings, SAE, and Metric seals.	set	8		
19	Mud seal "V"	pcs	4		
20	Pack of gasket for the Power units(Deck Engine, Carrier Truck Engine, welder Generator, booster Engine)- 1 set for each	Set	4		
21	Shear Pins & Fuses: For mechanical and electrical overload protection.	set	4		
22	BOP Seal Kit: Critical for maintaining the Blowout Preventer pressure integrity	set	4		
	Sub Total FCA 	
	Freight Cost ( For the Rigs + Spareparts+ Accessories +Tools)	
	Insurance cost	
	Customs clearance, and offloading cost  	
	PDI for the Truck  	
	Installation, and commissioning  of the Rig(The awarded bidder is required to commission the drilling Rig by drilling a 600mtr long drilling well) as per the required depth of max 600Mtr at final destination (Afar, Dire Dawa Administration ,Somali & Oromia) 	
	Training cost  at the Four Locations (Afar, Dire Dawa Administration Somali & Oromia) for 10 persons per / location for a duration of 20days-for each of the regions however the training is going to be made simultaneously. The Total Training Period for all the Regions should not exceed 30Days	
	Bidder’s Total prices DAP- MILS Warehouse (Total FCA+Freight Cost+ Insurance cost+ Customs clearance and offloading cost, PDI Cost , Installation , commissioning and Training Cost  at final destination)  	



Breakdown of Major Equipment 
No	Description	Qty	Currency USD
			Unit price	FCA (b)	Unit price	DAP (C)
1	Truck 6*6 or 8*4  for the 600 mtr drilling Rig 	1		
2	Deckengine- for the 600 mtr drilling Rig 	1		
3	Compressor for the 600 mtr drilling Rig 	1		
4	Mobile Compressor for the 600 mtr drilling Rig 	1		
5	Welder-Generator Set for the 600 mtr drilling Rig 	1		
6	Booster Machine for the 600 mtr drilling Rig 	1		
7	Triplex Mud Pump for the 600 mtr drilling Rig 	1		
8	Mud Pump for the 600 mtr drilling Rig 	1		
9	The Complete Drilling  Rig excluding (Booster machine,Mobile compressor and Tools, Accessories and Spareparts) which includes Mast, Hydraulic Clutch, outrigger, mud pumps, generator, compressor , winch and other  for the 600 mtr drilling Rig 	1		


 Budgetary Information for spareparts for Drilling Rig 600Mtr

No	Description	Unit	FCA Unit Price in USD
1	Recommended spare parts for Fast moving items for two years under continuous operations other than the above list of spare parts  shall be listed and offered financially not more than 2.5% of the rig cost. ( provide the list and attach separately with its unit and total price)		


Payment terms 30 days accepted: ☐ Yes
Bidder’s discount for accelerated payment: ____% of total firm price for each calendar day less than thirty (30) days 
Bidder’s delivery data  

Country of origin of offered products		
FCA point(s) of delivery for offered products		
Shipment dimensions of offered products (Including package)	Gross weight	Total volume	Containers (if applicable)
			Number	Size
				

I, the undersigned, certify that I am duly authorised by [insert full name of Bidder] to sign this quotation and bind [insert full name of Bidder] should UNOPS accept this quotation: 

Name	: _____________________________________________________________

Title	: _____________________________________________________________

Date	: _____________________________________________________________
Signature	: _____________________________________________________________













Lot 3-Drilling Rig 350mtr with  tools accessories and spareparts - 3 Units
ITB reference no: [insert ITB reference No.]
Name of Bidder: [insert name of bidder]

Bidders shall fill in these Price Schedule Forms in accordance with the instructions indicated.  
Bid Summary
It. No.	Description	UoM	Qty (a)	Currency USD
				Unit price FCA (b)	Total price FCA (c)= (a)x(b)
1	Complete set of Drilling rig 350mtr with truck, Mast, Outrigger, welder- generator, deckengine , mudpumps and compressor, 	Set	3		
Drilling Tools and Accessories for 350Mtr Drilling Rig
No.	Description	UNIT	Qty		
1	DRILL PIPE 5", length 6 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	195		
2	DRILL PIPE 5", length 3 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	6		
3	DRILL COLLAR 6" (152,4 mm) Length 3 m, thread 4 1/2" API REG, internal diameter 80 mm, wrench on both ends and thread protection.	PCS	6		
4	DRILL COLLAR 8" (203.2 mm) Length 6 m, thread 6 5/8" API REG, internal diameter 90 mm, wrench on both ends and thread protection with non return valve which are replaceable	PCS	6		
5	Spiral stabilizers 12 1/4" - body 8"x2 m with 6 5/8"API REG (B))x(P), wrench recess on both ends and hard thread protection	PCS	3		
6	Spiral stabilizers 14" (350 mm) - body 8" (203 mm) x1,5 m with 6 5/8"API REG (B))x(P), internal hole diameter 80 mm	PCS	6		
7	Cross over sub 4 1/2" API IF box x 3 1/2" API IF pin, length 300 mm	PCS	6		
8	Cross over sub 4 1/2" API IF box x 6 5/8"	PCS	3		
9	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 3 1/2" API IF, load capacity 3200 Kg	PCS	6		
10	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 6 5/8" API IF, load capacity 4600 Kg	PCS	6		
11	HOISTING PLUG, BOX type for drill rods with threads 4 1/2" API REG, load capacity 2000 Kg	PCS	6		
12	HOISTING PLUG, BOX type for drill rods with threads 6 5/8" API REG, load capacity 2000 Kg	PCS	3		
13	HOISTING PLUG, Box type, for drilling bits with threads 7 5/8" API REG, load capacity 4600 Kg	PCS	3		
14	SUB, 4 1/2" API REG BOX, 4 1/2" API REG BOX	PCS	6		
15	SUB, 6 5/8" API REG BOX, 6 5/8" API REG BOX	PCS	12		
16	SUB 3"1/2 API IF Box, 4"1/2 API REG Box	PCS	6		
17	SUB, 6 5/8" API REG BOX, 4 1/2" API REG BOX	PCS	6		
18	SUB, 6 5/8" API REG PIN, 4 1/2" API REG BOX	PCS	6		
19	SUB, 6 5/8" API REG BOX, 7 5/8" API REG BOX	PCS	3		
20	Drag bit 10 5/8" (270 mm), thread 4 1/2" API REG Pin	PCS	6		
21	Drag bit 14 3/4" (375 mm), thread 4 1/2" API REG Pin	PCS	3		
22	Drag bit 12 1/4" (311 mm), thread 3 1/2" API REG Pin	PCS	6		
23	Drag bit 17 1/2" (444,5 mm), thread 6 5/8" API REG Pin	PCS	3		
24	Tricone 12 1/4" (311.1 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "4", for medium-hard formation and 3 jet flushing	PCS	3		
25	Tricone 14 3/4" (374.6 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing		3		
26	TRICONE 17 1/2" (444.5 mm) IADC 535, TCI inserts, thread 7 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing	PCS	3		
27	TRICONE 9 7/8" (250,8 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for hard formation and central flushing	PCS	6		
28	TRICONE 9 7/8" (250,8 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	3		
29	TRICONE 12 1/4" (311,1 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	6		
30	TRICONE 14 3/4" (375 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	3		
31	TRICONE 17 1/2" (444,5 mm) IADC 211, tooth type, thread 7 5/8" API REG Pin, for soft formation and with central flushing	PCS	3		
32	SHOCK ABSORBER for DTH HAMMER 12", thread 6 5/8" API Reg	PCS	6		
33	SHOCK ABSORBER for DTH HAMMER 8", thread 4 1/2" API Reg	PCS	3		
34	SHOCK ABSORBER for DTH HAMMER 10", thread 6 5/8" API Reg	PCS	6		
35	DOWN THE HOLE HAMMER 10" with shank SD 10 and thread 6 5/8" API REG Pin	PCS	3		
36	DOWN THE HOLE HAMMER 8" with shank DHD 380 and thread 4 1/2" API REG Pin	PCS	3		
37	DOWN THE HOLE HAMMER 12" with shank SD 12 and thread 6 5/8" API REG Pin	PCS	6		
38	BIT 12 1/4" (311 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	6		
39	BIT 10" (254 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	6		
40	BIT 15" (381 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	3		
41	BIT 8 1/2" (216 mm) concave face for DTH Hammer 8" with shank DHD 380	PCS	3		
42	BIT 10" (254 mm) concave face for DTH Hammer 8" with shank DHD 380	PCS	6		
43	BIT 12 1/4" (311 mm) concave face for DTH Hammer 8" with shank DHD 380	PCS	6		
44	BIT 12 1/4" (311 mm) concave face for DTH Hammer 12" with shank SD 12	PCS	6		
45	BIT 17 1/2" (445 mm) concave face for DTH Hammer 12" with shank SD 12	PCS	3		
46	Steel Casing elevators 6 5/8"	PCS	6		
47	Steel Casing elevators 8 5/8"	PCS	6		
48	Steel Casing elevators 10 3/4"	PCS	6		
49	Steel Casing elevators 17 1/2"	PCS	6		
50	Steel Casing elevators 121/2"	PCS	6		
51	Steel Casing elevators 141/2"	PCS	3		
52	Loading kit (2 cable rings plus 2 shackles) for casing elevator, max capacity 30 tons	Set	3		
53	Casing clamp and slips for steel casing 6 5/8", max capacity 55 tons	PCS	3		
54	Casing clamp and slips for steel casing 8 5/8", max capacity 20 tons	PCS	3		
55	Casing clamp and slips for steel casing 10 3/4", max capacity 55 tons	PCS	3		
56	Casing clamp and slips for steel casing 12 3/4", max capacity 55 tons	Pcs	3		
57	Casing clamp and slips for steel casing 14 3/4", max capacity 55 tons	Pcs	3		
58	Casing Elevators for 6 5/8" PVC Casing	PCS	3		
59	Casing Elevators for 8 5/8" PVC Casing	PCS	3		
60	Casing Elevators for 10 3/4" PVC Casing	PCS	3		
61	Kit of casing clamp for 6 5/8", " PVC casing flush joint type (n°1 each diameter)	PCS	3		
62	Kit of casing clamp for 8 5/8", PVC casing flush joint type (n°1 each diameter)	PCS	3		
63	Kit of casing clamp for 10 3/4" PVC casing flush joint type (n°1 each diameter)	PCS	3		
64	Fishing tools with:	= taper tap for 3 1/2" API IF Box drill pipe, -1pcs each	= die collar for 3 1/2" API IF Box drill pipe, -1pcseach	= fishing magnet OD 6 1/2" with pulling capacity 400kg-1pcseach	Set	3		
65	JET HOOPER MIXER: Jet hopper mixer 60 liters with accessories.	Pcs	3		
66	Foldable Water tight canvas TANK FOR FOAM and WATER: Minimum Capacity of 1000litrs,	with air agitation for polymer mixing.	Pcs	3		
67	HAND OPERATED manual OIL & FUEL pump	Filling pump with filter for oil & fuel, actioned manually.	Pcs	3		
68	Top adaptor spanner for DTH hammer cylinder 8"	Pcs	3		
69	TOP ADAPTOR SPANNER	Pcs	3		
70	14" BIT SPANNER	Pcs	3		
71	12" BIT SPANNER	Pcs	3		
72	10" BIT SPANNER	Pcs	3		
73	8" BIT SPANNER	Pcs	3		
74	17 1/2" Bit spanner	Pcs	3		
75	Standard safety equipment for a crew of six members	Set	18		
	TOOL BOX & MAINTENANCE KIT	
	Description	Unit	 Qty		
1	Slogging Wrenches: Open-end and 12-point box ends (up to 3" or 75mm) for hammer-tightening structural bolts.	set	3		
2	Heavy-Duty Socket Set: 3/4" and 1" drive sets for high-torque applications.	set	3		
3	Torque Multipliers: Essential for reaching the high foot-pound requirements of flange bolts and mounting hardware.	set	3		
4	Large Pipe Wrenches: 18 ", 24", 36", and 48" (Rigid-style) for mud lines and drill floor piping.(each size 1 pcs)	set	3		
5	Impact Wrenches: Pneumatic 1" drive impact tools for fast removal of heavy covers and guards.	pcs	3		
6	Pressure Gauges: 0–5,000 psi (350 bar) digital or liquid-filled gauges with quick-connect fittings.	pcs	3		
7	Hydraulic Hose Crimper & Cutter: For on-site repairs of auxiliary lines.	set	3		
8	Hydraulic Jacks: 20-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	3		
9	Hydraulic Jacks: 50-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	3		
10	Fluid Sampling Kit: To monitor hydraulic oil cleanliness and prevent pump cavitation.-	set	3		
11	Digital Mustimeter: CAT IV rated (e.g., Fluke 87V or equivalent) for troubleshooting high-voltage power systems.	pcs	3		
12	Clamp Meter: To measure high amperage on mud pump motors and the drawworks.	pcs	3		
13	Insulation Tester (Megohmmeter): For testing motor windings and cable integrity against the rig ground.	pcs	3		
14	Precision Screwdriver Set: For PLC (Programmable Logic Controller) and control board wiring.	set	3		
15	Infrared (Thermal) Camera: To detect hot spots in electrical panels or overheating bearings before they fail.	set	3		
16	High-Pressure Grease Gun: Manual and battery-powered (18V) for the dozens of grease points on the mast and swivel.	pcs	3		
17	Lubrication Chart: Specific to your rig model, tracking hours vs. grease type (EP2, High-Temp, etc.).	pcs	3		
18	Oil Filter Wrenches: Large strap-style wrenches for engine and hydraulic return filters.	pcs	3		
19	Parts Washer/Solvent Kit: For cleaning shale shaker screens and fouled valves.	pcs	3		
	Spare parts to be supplied for the 350M Drilling Rig	
	Description	Unit	 Qty		
1	Truck air filter set	pcs	15		
2	Truck oil filter set	pcs	30		
3	Truck fuel filter set	pcs	30		
4	Deck engine air filters	pcs	15		
5	Deck engine oil filters	pcs	30		
6	Deck engine fuel filters	pcs	30		
7	welder Generator air filters	pcs	15		
8	welder Generator oil filters	pcs	30		
9	welder Generator fuel filters	pcs	30		
10	V-Belts: A matched set for the cooling fans and auxiliary pumps for the primary power unit(Deck Engine, Carrier Truck Engine, welder Generator,)- 2Pcs for Each	Set	3		
11	Hydraulic oil filter elements set- for the hydraulic system	set	6		
12	Wheel and master cylinder repair kit & brake lining	pcs	15		
13	All hydraulic lines and hoses fitting seals (Washers and seal kit)	kit	30		
14	Kit for air compressor	kit	30		
15	Flange and O-Ring Kit: A comprehensive set of Viton O-rings, SAE, and Metric seals.	set	12		
16	Mud seal "V"	pcs	6		
17	Pack of gasket for the Power units(Deck Engine, Carrier Truck Engine, welder Generator, )- 1 set for each	Set	3		
18	Shear Pins & Fuses: For mechanical and electrical overload protection.	set	3		
19	BOP Seal Kit: Critical for maintaining the Blowout Preventer pressure integrity	set	3		
	Total FCA	
	Freight Cost ( For the Rigs + Spareparts+ Accessories +Tools)	
	Insurance cost	
	Customs clearance and  offloading cost 	
	PDI for the Truck  	
	Installation, and commissioning  of the Rig(The awarded bidder is required to commission the drilling Rig by drilling a 350mtr long drilling well) as per the required depth of max 350Mtr at final destination(Afar, Somali & Oromia)	
	Training cost  at the three  Locations (Afar, Somali & Oromia) for 10 persons per / location for a duration of 20days-/for each of the regions however the training is going to be made simultaneously. The Total Training Period for all the Regions should not exceed 20Days	
	Bidder’s Total prices DAP- MILS Warehouse (Total FCA+Freight Cost+ Insurance cost+ Customs clearance and offloading cost, PDI Cost , Installation , commissioning and Training Cost at final destination)  -Afar, Somali & Oromia	




Lot 4-Drilling Rig 350mtr with  tools accessories and spareparts - 2 Units

Bid Summary
It. No.	Description	UoM	Qty (a)	Currency USD
				Unit price FCA (b)	Total price FCA (c)= (a)x(b)
1	Complete set of Drilling rig 350mtr with truck, Mast, Outrigger, welder- generator, deckengine , mudpumps and compressor, 	Set	2		
Drilling Tools and Accessories for 350Mtr Drilling Rig
No.	Description	UNIT	Qty		
1	DRILL PIPE 5", length 6 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	130		
2	DRILL PIPE 5", length 3 m, Thread 3 1/2"API IF, pipe th. 8.8 (N80), length tool joints (42CrMo4) 300 and 250 mm, wrench recess on both joints and thread protection	PCS	4		
3	DRILL COLLAR 6" (152,4 mm) Length 3 m, thread 4 1/2" API REG, internal diameter 80 mm, wrench on both ends and thread protection.	PCS	4		
4	DRILL COLLAR 8" (203.2 mm) Length 6 m, thread 6 5/8" API REG, internal diameter 90 mm, wrench on both ends and thread protection with non return valve which are replaceable	PCS	4		
5	Spiral stabilizers 12 1/4" - body 8"x2 m with 6 5/8"API REG (B))x(P), wrench recess on both ends and hard thread protection	PCS	2		
6	Spiral stabilizers 14" (350 mm) - body 8" (203 mm) x1,5 m with 6 5/8"API REG (B))x(P), internal hole diameter 80 mm	PCS	4		
7	Cross over sub 4 1/2" API IF box x 3 1/2" API IF pin, length 300 mm	PCS	4		
8	Cross over sub 4 1/2" API IF box x 6 5/8"	PCS	2		
9	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 3 1/2" API IF, load capacity 3200 Kg	PCS	4		
10	HOISTING SWIVEL, BOX type, swivel type for drill rods with threads 6 5/8" API IF, load capacity 4600 Kg	PCS	4		
11	HOISTING PLUG, BOX type for drill rods with threads 4 1/2" API REG, load capacity 2000 Kg	PCS	4		
12	HOISTING PLUG, BOX type for drill rods with threads 6 5/8" API REG, load capacity 2000 Kg	PCS	2		
13	HOISTING PLUG, Box type, for drilling bits with threads 7 5/8" API REG, load capacity 4600 Kg	PCS	2		
14	SUB, 4 1/2" API REG BOX, 4 1/2" API REG BOX	PCS	4		
15	SUB, 6 5/8" API REG BOX, 6 5/8" API REG BOX	PCS	8		
16	SUB 3"1/2 API IF Box, 4"1/2 API REG Box	PCS	4		
17	SUB, 6 5/8" API REG BOX, 4 1/2" API REG BOX	PCS	4		
18	SUB, 6 5/8" API REG PIN, 4 1/2" API REG BOX	PCS	4		
19	SUB, 6 5/8" API REG BOX, 7 5/8" API REG BOX	PCS	2		
20	Drag bit 10 5/8" (270 mm), thread 4 1/2" API REG Pin	PCS	4		
21	Drag bit 14 3/4" (375 mm), thread 4 1/2" API REG Pin	PCS	2		
22	Drag bit 12 1/4" (311 mm), thread 3 1/2" API REG Pin	PCS	4		
23	Drag bit 17 1/2" (444,5 mm), thread 6 5/8" API REG Pin	PCS	2		
24	Tricone 12 1/4" (311.1 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "4", for medium-hard formation and 3 jet flushing	PCS	2		
25	Tricone 14 3/4" (374.6 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing		2		
26	TRICONE 17 1/2" (444.5 mm) IADC 535, TCI inserts, thread 7 5/8" API REG Pin, leg back protection type "3", for medium-hard formation and 3 jet flushing	PCS	2		
27	TRICONE 9 7/8" (250,8 mm) IADC 535, TCI inserts, thread 6 5/8" API REG Pin, leg back protection type "3", for hard formation and central flushing	PCS	4		
28	TRICONE 9 7/8" (250,8 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	2		
29	TRICONE 12 1/4" (311,1 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	4		
30	TRICONE 14 3/4" (375 mm) IADC 211, tooth type, thread 6 5/8" API REG Pin, for soft formation and with central flushing	PCS	2		
31	TRICONE 17 1/2" (444,5 mm) IADC 211, tooth type, thread 7 5/8" API REG Pin, for soft formation and with central flushing	PCS	2		
32	SHOCK ABSORBER for DTH HAMMER 12", thread 6 5/8" API Reg	PCS	4		
33	SHOCK ABSORBER for DTH HAMMER 8", thread 4 1/2" API Reg	PCS	2		
34	SHOCK ABSORBER for DTH HAMMER 10", thread 6 5/8" API Reg	PCS	4		
35	DOWN THE HOLE HAMMER 10" with shank SD 10 and thread 6 5/8" API REG Pin	PCS	2		
36	DOWN THE HOLE HAMMER 8" with shank DHD 380 and thread 4 1/2" API REG Pin	PCS	2		
37	DOWN THE HOLE HAMMER 12" with shank SD 12 and thread 6 5/8" API REG Pin	PCS	4		
38	BIT 12 1/4" (311 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	4		
39	BIT 10" (254 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	4		
40	BIT 15" (381 mm) concave face for DTH Hammer 10" with shank SD 10	PCS	2		
41	BIT 8 1/2" (216 mm) concave face for DTH Hammer 8" with shank DHD 380	PCS	2		
42	BIT 10" (254 mm) concave face for DTH Hammer 8" with shank DHD 380	PCS	4		
43	BIT 12 1/4" (311 mm) concave face for DTH Hammer 8" with shank DHD 380	PCS	4		
44	BIT 12 1/4" (311 mm) concave face for DTH Hammer 12" with shank SD 12	PCS	4		
45	BIT 17 1/2" (445 mm) concave face for DTH Hammer 12" with shank SD 12	PCS	2		
46	Steel Casing elevators 6 5/8"	PCS	4		
47	Steel Casing elevators 8 5/8"	PCS	4		
48	Steel Casing elevators 10 3/4"	PCS	4		
49	Steel Casing elevators 17 1/2"	PCS	4		
50	Steel Casing elevators 121/2"	PCS	4		
51	Steel Casing elevators 141/2"	PCS	2		
52	Loading kit (2 cable rings plus 2 shackles) for casing elevator, max capacity 30 tons	Set	2		
53	Casing clamp and slips for steel casing 6 5/8", max capacity 55 tons	PCS	2		
54	Casing clamp and slips for steel casing 8 5/8", max capacity 20 tons	PCS	2		
55	Casing clamp and slips for steel casing 10 3/4", max capacity 55 tons	PCS	2		
56	Casing clamp and slips for steel casing 12 3/4", max capacity 55 tons	Pcs	2		
57	Casing clamp and slips for steel casing 14 3/4", max capacity 55 tons	Pcs	2		
58	Casing Elevators for 6 5/8" PVC Casing	PCS	2		
59	Casing Elevators for 8 5/8" PVC Casing	PCS	2		
60	Casing Elevators for 10 3/4" PVC Casing	PCS	2		
61	Kit of casing clamp for 6 5/8", " PVC casing flush joint type (n°1 each diameter)	PCS	2		
62	Kit of casing clamp for 8 5/8", PVC casing flush joint type (n°1 each diameter)	PCS	2		
63	Kit of casing clamp for 10 3/4" PVC casing flush joint type (n°1 each diameter)	PCS	2		
64	Fishing tools with:	= taper tap for 3 1/2" API IF Box drill pipe, -1pcs each	= die collar for 3 1/2" API IF Box drill pipe, -1pcseach	= fishing magnet OD 6 1/2" with pulling capacity 400kg-1pcseach	Set	2		
65	JET HOOPER MIXER: Jet hopper mixer 60 liters with accessories.	Pcs	2		
66	Foldable Water tight canvas TANK FOR FOAM and WATER: Minimum Capacity of 1000litrs,	with air agitation for polymer mixing.	Pcs	2		
67	HAND OPERATED manual OIL & FUEL pump	Filling pump with filter for oil & fuel, actioned manually.	Pcs	2		
68	Top adaptor spanner for DTH hammer cylinder 8"	Pcs	2		
69	TOP ADAPTOR SPANNER	Pcs	2		
70	14" BIT SPANNER	Pcs	2		
71	12" BIT SPANNER	Pcs	2		
72	10" BIT SPANNER	Pcs	2		
73	8" BIT SPANNER	Pcs	2		
74	17 1/2" Bit spanner	Pcs	2		
75	Standard safety equipment for a crew of six members	Set	12		
	TOOL BOX & MAINTENANCE KIT	
	Description	Unit	 Qty		
1	Slogging Wrenches: Open-end and 12-point box ends (up to 3" or 75mm) for hammer-tightening structural bolts.	set	2		
2	Heavy-Duty Socket Set: 3/4" and 1" drive sets for high-torque applications.	set	2		
3	Torque Multipliers: Essential for reaching the high foot-pound requirements of flange bolts and mounting hardware.	set	2		
4	Large Pipe Wrenches: 18 ", 24", 36", and 48" (Rigid-style) for mud lines and drill floor piping.(each size 1 pcs)	set	2		
5	Impact Wrenches: Pneumatic 1" drive impact tools for fast removal of heavy covers and guards.	pcs	2		
6	Pressure Gauges: 0–5,000 psi (350 bar) digital or liquid-filled gauges with quick-connect fittings.	pcs	2		
7	Hydraulic Hose Crimper & Cutter: For on-site repairs of auxiliary lines.	set	2		
8	Hydraulic Jacks: 20-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	2		
9	Hydraulic Jacks: 50-ton "pancake" or bottle jacks for leveling or component lifting.	pcs	2		
10	Fluid Sampling Kit: To monitor hydraulic oil cleanliness and prevent pump cavitation.-	set	2		
11	Digital Mustimeter: CAT IV rated (e.g., Fluke 87V or equivalent) for troubleshooting high-voltage power systems.	pcs	2		
12	Clamp Meter: To measure high amperage on mud pump motors and the drawworks.	pcs	2		
13	Insulation Tester (Megohmmeter): For testing motor windings and cable integrity against the rig ground.	pcs	2		
14	Precision Screwdriver Set: For PLC (Programmable Logic Controller) and control board wiring.	set	2		
15	Infrared (Thermal) Camera: To detect hot spots in electrical panels or overheating bearings before they fail.	set	2		
16	High-Pressure Grease Gun: Manual and battery-powered (18V) for the dozens of grease points on the mast and swivel.	pcs	2		
17	Lubrication Chart: Specific to your rig model, tracking hours vs. grease type (EP2, High-Temp, etc.).	pcs	2		
18	Oil Filter Wrenches: Large strap-style wrenches for engine and hydraulic return filters.	pcs	2		
19	Parts Washer/Solvent Kit: For cleaning shale shaker screens and fouled valves.	pcs	2		
	Spare parts to be supplied for the 350M Drilling Rig	
	Description	Unit	 Qty		
1	Truck air filter set	pcs	10		
2	Truck oil filter set	pcs	20		
3	Truck fuel filter set	pcs	20		
4	Deck engine air filters	pcs	10		
5	Deck engine oil filters	pcs	20		
6	Deck engine fuel filters	pcs	20		
7	welder Generator air filters	pcs	10		
8	welder Generator oil filters	pcs	20		
9	welder Generator fuel filters	pcs	20		
10	V-Belts: A matched set for the cooling fans and auxiliary pumps for the primary power unit(Deck Engine, Carrier Truck Engine, welder Generator,)- 2Pcs for Each	Set	2		
11	Hydraulic oil filter elements set- for the hydraulic system	set	4		
12	Wheel and master cylinder repair kit & brake lining	pcs	10		
13	All hydraulic lines and hoses fitting seals (Washers and seal kit)	kit	20		
14	Kit for air compressor	kit	20		
15	Flange and O-Ring Kit: A comprehensive set of Viton O-rings, SAE, and Metric seals.	set	8		
16	Mud seal "V"	pcs	4		
17	Pack of gasket for the Power units(Deck Engine, Carrier Truck Engine, welder Generator, )- 1 set for each	Set	2		
18	Shear Pins & Fuses: For mechanical and electrical overload protection.	set	2		
19	BOP Seal Kit: Critical for maintaining the Blowout Preventer pressure integrity	set	2		
	Total FCA	
	Freight Cost ( For the Rigs + Spareparts+ Accessories +Tools)	
	Insurance cost	
	Customs clearance and  offloading cost 	
	PDI for the Truck  	
	Installation, and commissioning  of the Rig(The awarded bidder is required to commission the drilling Rig by drilling a 350mtr long drilling well) as per the required depth of max 350Mtr at final destination(Afar, Somali & Oromia)	
	Training cost  at the three  Locations (Afar, Somali & Oromia) for 10 persons per / location for a duration of 20days-/for each of the regions however the training is going to be made simultaneously. The Total Training Period for all the Regions should not exceed 20Days	
	Bidder’s Total prices DAP- MILS Warehouse (Total FCA+Freight Cost+ Insurance cost+ Customs clearance and offloading cost, PDI Cost , Installation , commissioning and Training Cost at final destination)  -Afar, Somali & Oromia	











Breakdown of Major Equipment 350mtr
No	Description	Qty	Currency USD
			Unit price	FCA (b)	Unit price	DAP (C)
1	Truck 6*6 or 8*4 axle for 350mtr drilling Rig 	1		
2	Deckengine 350mtr drilling Rig 	1		
3	Compressor- 350mtr drilling Rig 	1		
4	Triplex Mud Pump- 350mtr drilling Rig 	1		
5	Welder-Generator Set- 350mtr drilling Rig 	1		
6	Mud Pump-350mtr drilling Rig 	1		
7	The Complete  Rig which includes Mast, Hydraulic Clutch, outrigger, winch,etc excluding tools, accessories and spareparts.	1		




 Budgetary Information for spareparts for Drilling Rig 350Mtr

No	Description	Unit	FCA Unit Price in USD
1	Recommended spare parts for Fast moving items for two years under continuous operations other than the above list of spare parts  shall be listed and offered financially not more than 2.5% of the rig cost. ( provide the list and attach separately with its unit and total price)		

Payment terms 30 days accepted: ☐ Yes
Bidder’s discount for accelerated payment: ____% of total firm price for each calendar day less than thirty (30) days 
Bidder’s delivery data  

Country of origin of offered products		
FCA point(s) of delivery for offered products		
Shipment dimensions of offered products (Including package)	Gross weight	Total volume	Containers (if applicable)
			Number	Size
				

I, the undersigned, certify that I am duly authorised by [insert full name of Bidder] to sign this quotation and bind [insert full name of Bidder] should UNOPS accept this quotation: 

Name	: _____________________________________________________________

Title	: _____________________________________________________________

Date	: _____________________________________________________________

Signature	: _____________________________________________________________
Form D: Technical Bid Form
ITB reference no: [insert ITB reference No.]

Name of Bidder: [insert name of bidder]

Bidders are required to complete the Comparative Data Tables included in Section II: Schedule of Requirements to demonstrate compliance with UNOPS requirements and insert them below. Bidders are NOT allowed to make any change in the “UNOPS requirements” columns of the Comparative Data Tables. Such changes might disqualify your bid.


	Note to Bidders: 

1. Bidders are required to clearly complete the below detailed technical criteria for each proposed product.The specification of the proposed product must correspond with the UNOPS minimum requirements indicated in Section II (Schedule of Requirements) of this ITB.  i.e. for each product requirement listed below, the bidder must provide the corresponding specification  demonstrating alignment with the specified minimum technical requirement.   In the case of deviation, the bidder is to provide an additional explanation in the remarks column. Bidders are required to provide their technical bid submission on the excel sheet shared with the bid- Form D- Excel Version

2. The Bidder’s specification shall be consistent with the brand and model number indicated in the product data sheet / catalogue submitted.Bidders are requested to provide manufacturer’s product data sheet /catalogue to support the bidder’s proposed product specification. Failure to provide the proposed products’ technical details in this form may result in the disqualification of the bid.

3. For each item, the bidder must propose/indicate only one Brand, Model and Model no. Proposing/indicating more than one Brand, Model and Model is forbidden. 

N.B. Failure to comply with the above instructions may result in rejection of bids. 




Technical specifications for Goods – Comparative Data Table

Bidders must submit their technical bid in a separate document using Form D in Excel format, which is attached to the bid document (mandatory requirement)


















Form E: Performance Statement Form

ITB reference no: [insert ITB reference No.]
Name of Bidder: [insert name of bidder]
Date: [insert submission date]


	Order placed by (Full address of purchaser)
	Order no & date
	Description & quantity of ordered items
	Value of Order
	Date of completion of Delivery
	Remarks indicating reasons of late delivery, if any
	Was the supply of goods satisfactory?

	
	
	
	
	As per Contract
	Actual
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	





Name	: _____________________________________________________________

Title	: _____________________________________________________________

Date	: _____________________________________________________________

Signature	: _____________________________________________________________







Form F: Manufacturer’s Authorization Form

A letter issued by the manufacturer authorizing the applicant to participate in this particular ITB must be submitted with the bid in the format provided in this Form. 

To be eligible for delivery of goods, the bidder must be either the manufacturer of the offered goods or a sole representative of the manufacturer to the United Nations. Should offers for a particular make and model be received from more than one appointed representative, UNOPS reserves the right to select only one.


ITB reference no: [insert ITB reference No.]
Name of Bidder: [insert name of bidder]
Date: [insert submission date]

To: UNOPS 


WHEREAS


We [insert complete name of manufacturer], who are official manufacturers of [insert type of goods manufactured], having factories at [insert full address of manufacturer’s factories], do hereby authorize [insert complete name of bidder] to submit a bid the purpose of which is to provide the following goods, manufactured by us [insert name and or brief description of the goods], and to subsequently negotiate and sign the contract.

We hereby extend our full guarantee and warranty in accordance with Clause 4.5 of the General Conditions of Contract for the provision of Goods, with respect to the goods offered by the above firm.

Signed: [insert signature(s) of authorized representative(s) of the manufacturer] 


Name: [insert complete name(s) of authorized representative(s) of the manufacturer]	

Title: [insert title] 



Dated on ____________ day of __________________, _______ [insert date of signing]
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